{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["TARIF JUILLET 2014"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TARIF JUILLET 2014","index":0,"n_rows":393,"n_cols":5,"rows_kept":393,"cut":false,"hidden":false,"merged":[[3,0,4,4],[12,0,21,0],[7,0,7,4],[127,0,127,4]]}
[]
[]
[]
["TARIF SERTINOXTM Edition Juillet 2014"]
[]
[]
[]
["Les raccords du diamètres 15mm au 54mm ont tous un film bleu sur le(s) bourrelet(s) à sertir et sont équipés de joints à sécurité, ces 2 éléments permettent de détecter rapidement un raccord non serti."]
[]
[]
[]
[null,"Référence","Libellé","P.U. H.T.","Condit."]
[null,"C 90 - 15","Courbe à 90° diamètre extérieur 15",6.5299999999999994,20]
[null,"C 90 - 18","Courbe à 90° diamètre extérieur 18",7.75,20]
[null,"C 90 - 22","Courbe à 90° diamètre extérieur 22",8.89,20]
[null,"C 90 - 28","Courbe à 90° diamètre extérieur 28",11.26,10]
[null,"C 90 - 35","Courbe à 90° diamètre extérieur 35",17.700000000000003,10]
[null,"C 90 - 42","Courbe à 90° diamètre extérieur 42",32.489999999999995,2]
[null,"C 90 - 54","Courbe à 90° diamètre extérieur 54",44.37,2]
[null,"C 90 - 76","Courbe à 90° diamètre extérieur 76",106.49000000000001,2]
[null,"C 90 - 89","Courbe à 90° diamètre extérieur 89",129.47,2]
[null,"C 90 - 108","Courbe à 90° diamètre extérieur 108",176.98999999999998,2]
[null,"CE 90 - 15","Courbe à emboîter à 90° diam. ext. 15",6.66,20]
[null,"CE 90 - 18","Courbe à emboîter à 90° diam. ext. 18",7.59,20]
[null,"CE 90 - 22","Courbe à emboîter à 90° diam. ext. 22",8.8699999999999992,20]
[null,"CE 90 - 28","Courbe à emboîter à 90° diam. ext. 28",11.07,10]
[null,"CE 90 - 35","Courbe à emboîter à 90° diam. ext. 35",17.37,10]
[null,"CE 90 - 42","Courbe à emboîter à 90° diam. ext. 42",30.970000000000002,2]
[null,"CE 90 - 54","Courbe à emboîter à 90° diam. ext. 54",43.04,2]
[null,"CE 90 - 76","Courbe à emboîter à 90° diam. ext. 76",106.49000000000001,2]
[null,"CE 90 - 89","Courbe à emboîter à 90° diam. ext. 89",129.47,2]
[null,"CE 90 - 108","Courbe à emboîter à 90° diam. ext. 108",176.98999999999998,2]
[null,"CA90 - 15","Coude d'ajustage à 90° diam. ext. 15",7.97,20]
[null,"CA90 - 18","Coude d'ajustage à 90° diam. ext. 18",8.11,20]
[null,"CA90 - 22","Coude d'ajustage à 90° diam. ext. 22",8.52,10]
[null,"CA90 - 28","Coude d'ajustage à 90° diam. ext. 28",11.06,10]
[null,"CA90 - 35","Coude d'ajustage à 90° diam. ext. 35",18.540000000000003,4]
[null,"CA90 - 42","Coude d'ajustage à 90° diam. ext. 42",23.48,2]
[null,"CA90 - 54","Coude d'ajustage à 90° diam. ext. 54",29.400000000000002,2]
[null,"CA90 - 76","Coude d'ajustage à 90° diam. ext. 76",101.55000000000001,2]
[null,"CA90 - 89","Coude d'ajustage à 90° diam. ext. 89",121.03,2]
[null,"CA90 - 108","Coude d'ajustage à 90° diam. ext. 108",156.5,2]
[null,"C45 - 15","Coude à 45° diam. ext. 15",8.8699999999999992,20]
[null,"C45 - 18","Coude à 45° diam. ext. 18",9.4700000000000006,20]
[null,"C45 - 22","Coude à 45° diam. ext. 22",11.02,20]
[null,"C45 - 28","Coude à 45° diam. ext. 28",12.85,10]
[null,"C45 - 35","Coude à 45° diam. ext. 35",16.53,10]
[null,"C45 - 42","Coude à 45° diam. ext. 42",26.59,4]
[null,"C45 - 54","Coude à 45° diam. ext. 54",34.53,2]
[null,"C 45 - 76","Courbe à 45° diamètre extérieur 76",101.62,2]
[null,"C 45 - 89","Courbe à 45° diamètre extérieur 89",121.28,2]
[null,"C 45 - 108","Courbe à 45° diamètre extérieur 108",165.54,2]
[null,"CE45 - 15","Coude à emboîter à 45° diam. ext. 15",8.92,20]
[null,"CE45 - 18","Coude à emboîter à 45° diam. ext. 18",9.48,20]
[null,"CE45 - 22","Coude à emboîter à 45° diam. ext. 22",10.91,20]
[null,"CE45 - 28","Coude à emboîter à 45° diam. ext. 28",12.81,10]
[null,"CE45 - 35","Coude à emboîter à 45° diam. ext. 35",15.6,10]
[null,"CE45 - 42","Coude à emboîter à 45° diam. ext. 42",25.16,4]
[null,"CE45 - 54","Coude à emboîter à 45° diam. ext. 54",32.75,2]
[null,"CE 45 - 76","Courbe à emboîter à 45° diam. ext. 76",93.4,2]
[null,"CE 45 - 89","Courbe à emboîter à 45° diam. ext. 89",111.47,2]
[null,"CE 45 - 108","Courbe à emboîter à 45° diam. ext. 108",152.45999999999998,2]
[null,"CMF90 - 15.½","Courbe mixte fem. à 90° diam. ext. 15.½\"",15.39,20]
[null,"CMF90 - 18.½","Courbe mixte fem. à 90° diam. ext. 18.½\"",17.73,20]
[null,"CMF90 - 22.¾","Courbe mixte fem. à 90° diam. ext. 22.¾\"",18.739999999999998,10]
[null,"CMF90 - 28.1","Courbe mixte fem. à 90° diam. ext. 28.1\"",24.650000000000002,10]
[null,"CMF90 - 35.1¼ ","Courbe mixte fem. à 90° diam. ext. 35.1¼\"",33.03,10]
[null,"CMM90 - 15.½","Courbe mixte mâle à 90° diam. ext . 15.½\"",15.67,20]
[null,"CMM90 - 18.½","Courbe mixte mâle à 90° diam. ext. 18.½\"",16.28,20]
[null,"CMM90 - 22.¾","Courbe mixte mâle à 90° diam. ext. 22.¾\"",20.330000000000002,10]
[null,"CMM90 - 28.1","Courbe mixte mâle à 90° diam. ext. 28.1\"",24.32,10]
[null,"CMM90 - 35.1¼ ","Courbe mixte mâle à 90° diam. ext.  35.1¼\"",30.98,10]
[null,"CMM90 - 42.1½","Courbe mixte mâle à 90° diam. ext. 42.1½\"",48.11,2]
[null,"CMM90 - 54.2","Courbe mixte mâle à 90° diam. ext. 54.2\"",62.76,2]
[null,"CMM45 - 15.½","Courbe mixte mâle à 45° diam. ext . 15.½\"",16.57,20]
[null,"CMM45 - 18.½","Courbe mixte mâle à 45° diam. ext. 18.½\"",17.180000000000003,20]
[null,"CMM45 - 22.¾","Courbe mixte mâle à 45° diam. ext. 22.¾\"",21.34,10]
[null,"TE - 15","Té égal diam. ext. 15",11.4,20]
[null,"TE - 18","Té égal diam. ext. 18",11.879999999999999,20]
[null,"TE - 22","Té égal diam. ext. 22",13.61,20]
[null,"TE - 28","Té égal diam. ext. 28",15.959999999999999,10]
[null,"TE - 35","Té égal diam. ext. 35",21.430000000000003,10]
[null,"TE - 42","Té égal diam. ext. 42",29.950000000000003,4]
[null,"TE - 54","Té égal diam. ext. 54",35.44,2]
[null,"TE - 76","Té égal diam. ext. 76",191.75,2]
[null,"TE - 89","Té égal diam. ext. 89",209.79999999999998,2]
[null,"TE - 108","Té égal diam. ext. 108",258.90999999999997,2]
[null,"TR - 18.15.18","Té réduit diam. ext. 18 . 15 . 18",13.33,20]
[null,"TR - 22.15.22","Té réduit diam. ext. 22 . 15 . 22",12.92,20]
[null,"TR - 22.18.22","Té réduit diam. ext. 22 . 18 . 22",13.33,20]
[null,"TR - 28.15.28","Té réduit diam. ext. 28 . 15 . 28",13.47,10]
[null,"TR - 28.18.28","Té réduit diam. ext. 28 . 18 . 28",14.33,10]
[null,"TR - 28.22.28","Té réduit diam. ext. 28 . 22 . 28",15.1,10]
[null,"TR - 35.15.35","Té réduit diam. ext. 35 . 15 . 35",16.900000000000002,10]
[null,"TR - 35.18.35","Té réduit diam. ext. 35 . 18 . 35",17.290000000000003,10]
[null,"TR - 35.22.35","Té réduit diam. ext. 35 . 22 . 35",18.130000000000003,10]
[null,"TR - 35.28.35","Té réduit diam. ext. 35 . 28 . 35",18.940000000000001,10]
[null,"TR - 42.15.42","Té réduit diam. ext. 42 . 15 . 42",23.220000000000002,4]
[null,"TR - 42.18.42","Té réduit diam. ext. 42 . 18 . 42",24.17,4]
[null,"TR - 42.22.42","Té réduit diam. ext. 42 . 22 . 42",25,4]
[null,"TR - 42.28.42","Té réduit diam. ext. 42 . 28 . 42",25.94,4]
[null,"TR - 42.35.42","Té réduit diam. ext. 42 . 35 . 42",27.34,4]
[null,"TR - 54.15.54","Té réduit diam. ext. 54 . 15 . 54",28.830000000000002,2]
[null,"TR - 54.18.54","Té réduit diam. ext. 54 . 18 . 54",29.220000000000002,2]
[null,"TR - 54.22.54","Té réduit diam. ext. 54 . 22 . 54",29.880000000000003,2]
[null,"TR - 54.28.54","Té réduit diam. ext. 54 . 28 . 54",30.44,2]
[null,"TR - 54.35.54","Té réduit diam. ext. 54 . 35 . 54",31.28,2]
[null,"TR - 54.42.54","Té réduit diam. ext. 54 . 42 . 54",32.18,2]
[null,"TR - 76.22.76","Té réduit diam. ext. 76.22.76",144.22999999999999,2]
[null,"TR - 76.28.76","Té réduit diam. ext. 76.28.76",155.67999999999998,2]
[null,"TR - 76.35.76","Té réduit diam. ext. 76.35.76",167.14999999999998,2]
[null,"TR - 76.42.76","Té réduit diam. ext. 76.42.76",180.26999999999998,2]
[null,"TR - 76.54.76","Té réduit diam. ext. 76.54.76",191.75,2]
[null,"TR - 89.22.89","Té réduit diam. ext. 89.22.89",152.45999999999998,2]
[null,"TR - 89.28.89","Té réduit diam. ext. 89.28.89",163.87,2]
[null,"TR - 89.35.89","Té réduit diam. ext. 89.35.89",175.32,2]
[null,"TR - 89.42.89","Té réduit diam. ext. 89.42.89",188.47,2]
[null,"TR - 89.54.89","Té réduit diam. ext. 89.54.89",196.66,2]
[null,"TR - 89.76.89","Té réduit diam. ext. 89.76.89",209.79999999999998,2]
[null,"TR - 108.22.108","Té réduit diam. ext. 108.22.108",162.23999999999998,2]
[null,"TR - 108.28.108","Té réduit diam. ext. 108.28.108",172.04,2]
[null,"TR - 108.35.108","Té réduit diam. ext. 108.35.108",188.47,2]
[null,"TR - 108.42.108","Té réduit diam. ext. 108.42.108",196.66,2]
[null,"TR - 108.54.108","Té réduit diam. ext. 108.54.108",213.07999999999998,2]
[null,"TR - 108.76.108","Té réduit diam. ext. 108.76.108",224.51,2]
[null,"TR - 108.89.108","Té réduit diam. ext. 108.89.108",257.33999999999997,2]
[]
["TÉ MIXTE FEMELLE"]
[]
[null,"Référence","Libellé","P.U. H.T.","Condit."]
[null,"TMF - 15.½.15","Té mixte femelle diam. ext. 15.½\".15",13.87,20]
[null,"TMF - 18.½.18","Té mixte femelle diam. ext. 18.½\".18",14.43,20]
[null,"TMF - 22.½.22","Té mixte femelle diam. ext. 22.½\".22",14.98,20]
[null,"TMF - 28.½.28","Té mixte femelle diam. ext. 28.½\".28",17.170000000000002,10]
[null,"TMF - 35.½.35","Té mixte femelle diam. ext. 35.½\".35",19.790000000000003,10]
[null,"TMF - 42.½.42","Té mixte femelle diam. ext. 42.½\".42",24.040000000000003,4]
[null,"TMF - 54.½.54","Té mixte femelle diam. ext. 54.½\".54",27.200000000000003,2]
[null,"TMF - 18.¾.18","Té mixte femelle diam. ext. 18.¾\".18",14.98,20]
[null,"TMF - 22.¾.22","Té mixte femelle diam. ext. 22.¾\".22",16.350000000000001,20]
[null,"TMF - 28.¾.28","Té mixte femelle diam. ext. 28.¾\".28",17.950000000000003,10]
[null,"TMF - 35.¾.35","Té mixte femelle diam. ext. 35.¾\".35",22.26,10]
[null,"TMF - 42.¾.42","Té mixte femelle diam. ext. 42.¾\".42",29.540000000000003,4]
[null,"TMF - 54.¾.54","Té mixte femelle diam. ext. 54.¾\".54",33.659999999999997,2]
[null,"TMF - 76.¾.76","Té mixte femelle diam. ext. 76.¾\".76",156.91999999999999,2]
[null,"TMF - 89.¾.89","Té mixte femelle diam. ext. 89.¾\".89",170.51,2]
[null,"TMF - 108.¾.108","Té mixte femelle diam. ext. 108.¾\".108",205.17,2]
[null,"TMF - 28.1.28","Té mixte femelle diam. ext. 28.1\".28",21.630000000000003,10]
[null,"TMF - 35.1¼.35","Té mixte femelle diam. ext. 35.1¼\".35",27.200000000000003,10]
[null,"TMF - 42.1½.42","Té mixte femelle diam. ext. 42.1½\".42",30.91,10]
[null,"TMF - 54.2.54","Té mixte femelle diam. ext. 54.2\".54",52.98,2]
[null,"TMF - 76.2.76","Té mixte femelle diam. ext. 76.2\".76",173.48,2]
[null,"TMF - 89.2.90","Té mixte femelle diam. ext. 89.2\".89",181.07999999999998,2]
[null,"TMF - 108.2.108","Té mixte femelle diam. ext. 108.2\".108",218.79,2]
[null,"RMM - 15.⅜","Raccord mixte mâle diam. ext. 15.⅜\"",8.9,20]
[null,"RMM - 15.½","Raccord mixte mâle diam. ext. 15.½\"",9.75,20]
[null,"RMM - 15.¾","Raccord mixte mâle diam. ext. 15.¾\"",9.16,20]
[null,"RMM - 18.½","Raccord mixte mâle diam. ext. 18.½\"",9.91,20]
[null,"RMM - 18.¾","Raccord mixte mâle diam. ext. 18.¾\"",9.84,20]
[null,"RMM - 22.½","Raccord mixte mâle diam. ext. 22.½\"",10.68,20]
[null,"RMM - 22.¾","Raccord mixte mâle diam. ext. 22.¾\"",11.22,20]
[null,"RMM - 22.1","Raccord mixte mâle diam. ext. 22.1\"",13.87,20]
[null,"RMM - 28.¾","Raccord mixte mâle diam. ext. 28.¾\"",13.68,20]
[null,"RMM - 28.1","Raccord mixte mâle diam. ext. 28.1\"",14.209999999999999,20]
[null,"RMM - 28.1¼","Raccord mixte mâle diam. ext. 28.1¼\"",19.790000000000003,20]
[null,"RMM - 35.1","Raccord mixte mâle diam. ext. 35. 1\"",18.04,10]
[null,"RMM - 35.1¼","Raccord mixte mâle diam. ext. 35. 1¼\"",20.810000000000002,10]
[null,"RMM - 35.1½","Raccord mixte mâle diam. ext. 35.1½\"",24.060000000000002,10]
[null,"RMM - 42.1¼","Raccord mixte mâle diam. ext. 42. 1¼\"",27.32,4]
[null,"RMM - 42.1½","Raccord mixte mâle diam. ext. 42.1½\"",30.34,4]
[null,"RMM - 54.1½","Raccord mixte mâle diam. ext. 54.1½\"",38.28,4]
[null,"RMM - 54.2","Raccord mixte mâle diam. ext. 54.2\"",40.739999999999995,4]
[null,"RMM - 76.2½","Raccord mixte mâle diam. ext. 76.2½\"",189.06,2]
[null,"RMM - 89.3","Raccord mixte mâle diam. ext. 89.3\"",283.64999999999998,2]
[null,"RMF - 15.½","Raccord mixte femelle diam. ext. 15.½\"",9.6999999999999993,20]
[null,"RMF - 15.¾","Raccord mixte femelle diam. ext. 15.¾\"",10.1,20]
[null,"RMF - 18.½","Raccord mixte femelle diam. ext. 18.½\"",10.24,20]
[null,"RMF - 18.¾","Raccord mixte femelle diam. ext. 18.¾\"",10.68,20]
[null,"RMF - 22.½","Raccord mixte femelle diam. ext. 22.½\"",10.92,20]
[null,"RMF - 22.¾","Raccord mixte femelle diam. ext. 22.¾\"",12.86,20]
[null,"RMF - 22.1","Raccord mixte femelle diam. ext. 22.1\"",14.64,20]
[null,"RMF - 28.¾","Raccord mixte femelle diam. ext. 28.¾\"",13.93,20]
[null,"RMF - 28.1","Raccord mixte femelle diam. ext. 28.1\"",19.970000000000002,20]
[null,"RMF - 28.1¼","Raccord mixte femelle diam. ext. 28.1¼\"",22.130000000000003,20]
[null,"RMF - 35.1","Raccord mixte femelle diam. ext. 35.1 \"",19.12,10]
[null,"RMF - 35.1¼","Raccord mixte femelle diam. ext. 35.1¼ \"",21.85,10]
[null,"RMF - 35.1½","Raccord mixte femelle diam. ext. 35.1½ \"",24.880000000000003,10]
[null,"RMF - 42.1¼","Raccord mixte femelle diam. ext. 42.1¼ \"",29.540000000000003,4]
[null,"RMF - 42.1½","Raccord mixte femelle diam. ext. 42.1½\"",33.619999999999997,4]
[null,"RMF - 54.1½","Raccord mixte femelle diam. ext. 54.1½\"",36.919999999999995,4]
[null,"RMF - 54.2","Raccord mixte femelle diam. ext. 54.2\"",50.28,4]
[null,"R3M - 15.½","Raccord mixte 3 pièces mâle dia. ext. 15.½\"",18.04,20]
[null,"R3M - 15.¾","Raccord mixte 3 pièces mâle dia. ext. 15.¾\"",19.060000000000002,20]
[null,"R3M - 18.½","Raccord mixte 3 pièces mâle dia. ext. 18.½\"",19.87,20]
[null,"R3M - 18.¾","Raccord mixte 3 pièces mâle dia. ext. 18.¾\"",20.170000000000002,20]
[null,"R3M - 22.½","Raccord mixte 3 pièces mâle dia. ext. 22.½\"",24.26,20]
[null,"R3M - 22.¾","Raccord mixte 3 pièces mâle dia. ext. 22.¾\"",21.19,20]
[null,"R3M - 22.1","Raccord mixte 3 pièces mâle dia. ext. 22.1\"",29.8,20]
[null,"R3M - 28.1","Raccord mixte 3 pièces mâle dia. ext. 28.1\"",35.57,20]
[null,"R3M - 35.1¼","Raccord mixte 3 pièces mâle dia. ext. 35.1¼\"",45.35,10]
[null,"R3M - 42.1½","Raccord mixte 3 pièces mâle dia. ext. 42.1½\"",56.32,4]
[null,"R3M - 54.2","Raccord mixte 3 pièces mâle dia. ext. 54.2\"",90.64,4]
[null,"(Existe avec écrou tournant inox : nous consulter)"]
[]
[null,"R3F - 15.½","Raccord mixte 3 pièces femelle dia. ext. 15.½\"",17.760000000000002,20]
[null,"R3F - 15.¾","Raccord mixte 3 pièces femelle dia. ext. 15.¾\"",19.73,20]
[null,"R3F - 18.½","Raccord mixte 3 pièces femelle dia. ext. 18.½\"",21.400000000000002,20]
[null,"R3F - 18.¾","Raccord mixte 3 pièces femelle dia. ext. 18.¾\"",22.060000000000002,20]
[null,"R3F - 22.¾","Raccord mixte 3 pièces femelle dia. ext. 22.¾\"",23.67,20]
[null,"R3F - 22.1","Raccord mixte 3 pièces femelle dia. ext. 22.1\"",28.35,20]
[null,"R3F - 28.1","Raccord mixte 3 pièces femelle dia. ext. 28.1\"",30.740000000000002,20]
[null,"R3F - 35.1¼","Raccord mixte 3 pièces femelle dia. ext. 35.1¼\"",38.489999999999995,10]
[null,"R3F - 42.1½","Raccord mixte 3 pièces femelle dia. ext. 42.1½\"",47.48,4]
[null,"R3F - 54.2","Raccord mixte 3 pièces femelle dia. ext. 54.2\"",89.84,4]
[null,"RMB - 42.DN40","Raccord mixte à bride diam. ext. 42.DN40 PN16",124.99000000000001,2]
[null,"RMB - 54.DN50","Raccord mixte à bride diam. ext. 54.DN50 PN16",159.32999999999998,2]
[null,"RMB - 76.DN65","Raccord mixte à bride diam. ext. 76.DN65 PN16",210.14999999999998,2]
[null,"RMB - 89.DN80","Raccord mixte à bride diam. ext. 89.DN80 PN16",254.1,2]
[null,"RMB - 108.DN100","Raccord mixte à bride diam. ext. 108.DN100 PN16",302.17,2]
[null,"RMBF - 76","Raccord mixte à bride folle diam. ext. 76.DN65 PN10",125.05,2]
[null,"RMBF - 89","Raccord mixte à bride folle diam. ext. 89.DN80 PN10",138.38,2]
[null,"RMBF - 108","Raccord mixte à bride folle diam. ext. 108.DN100 PN10",164,2]
[null,"EMBF - 76","Embout mixte à bride folle diam. ext. 76.DN65 PN10",97.38000000000001,2]
[null,"EMBF - 89","Embout mixte à bride folle diam. ext. 89.DN80 PN10",106.6,2]
[null,"EMBF - 108","Embout mixte à bride folle diam. ext. 108.DN100 PN10",128.13,2]
[null,"M - 15","Manchon diamètre extérieur 15",4.59,20]
[null,"M - 18","Manchon diamètre extérieur 18",4.91,20]
[null,"M - 22","Manchon diamètre extérieur 22",5.95,20]
[null,"M - 28","Manchon diamètre extérieur 28",7.12,20]
[null,"M - 35","Manchon diamètre extérieur 35",8.26,10]
[null,"M - 42","Manchon diamètre extérieur 42",10.72,4]
[null,"M - 54","Manchon diamètre extérieur 54",13.51,4]
[null,"M - 76","Manchon diamètre extérieur 76",68.81,2]
[null,"M - 89","Manchon diamètre extérieur 89",78.64,2]
[null,"M - 108","Manchon diamètre extérieur 108",99.95,2]
[null,"MA - 15","Manchon d'ajustage diamètre extérieur 15",7.5299999999999994,20]
[null,"MA - 18","Manchon d'ajustage diamètre extérieur 18",7.84,20]
[null,"MA - 22","Manchon d'ajustage diamètre extérieur 22",8.89,20]
[null,"MA - 28","Manchon d'ajustage diamètre extérieur 28",10.44,20]
[null,"MA - 35","Manchon d'ajustage diamètre extérieur 35",11.66,10]
[null,"MA - 42","Manchon d'ajustage diamètre extérieur 42",13.49,4]
[null,"MA - 54","Manchon d'ajustage diamètre extérieur 54",17.180000000000003,4]
[null,"MA - 76","Manchon d'ajustage diamètre extérieur 76",101.62,2]
[null,"MA - 89","Manchon d'ajustage diamètre extérieur 89",114.73,2]
[null,"MA - 108","Manchon d'ajustage diamètre extérieur 108",137.66,2]
[null,"MFL - 15","Manchon d'extrémité diam. ext. 15",6.62,20]
[null,"MFL - 18","Manchon d'extrémité diam. ext. 18",6.92,20]
[null,"MFL - 22","Manchon d'extrémité diam. ext. 22",7.5299999999999994,20]
[null,"MFL- 28","Manchon d'extrémité diam. ext. 28",9.98,20]
[null,"MFL - 35","Manchon d'extrémité diam. ext. 35",11.209999999999999,10]
[null,"MFL - 42","Manchon d'extrémité diam. ext. 42",15.66,4]
[null,"MFL - 54","Manchon d'extrémité diam. ext. 54",18.110000000000003,4]
[null,"MFL - 76","Manchon d'extrémité diamètre extérieur 76",42.58,2]
[null,"MFL - 89","Manchon d'extrémité diamètre extérieur 89",56.32,2]
[null,"MFL - 108","Manchon d'extrémité diamètre extérieur 108",70.050000000000011,2]
[null,"RR - 18.15","Raccord de réduction diam. ext. 18.15",5.3199999999999994,20]
[null,"RR - 22.15","Raccord de réduction diam. ext. 22.15",5.7799999999999994,20]
[null,"RR - 22.18","Raccord de réduction diam. ext. 22.18",6.13,20]
[null,"RR - 28.15","Raccord de réduction diam. ext. 28.15",7.43,20]
[null,"RR - 28.18","Raccord de réduction diam. ext. 28.18",7.2799999999999994,20]
[null,"RR - 28.22","Raccord de réduction diam. ext. 28.22",7.56,20]
[null,"RR - 35.15","Raccord de réduction diam. ext. 35.15",14.1,10]
[null,"RR - 35.18","Raccord de réduction diam. ext. 35.18",14.54,10]
[null,"RR - 35.22","Raccord de réduction diam. ext. 35.22",9.49,10]
[null,"RR - 35.28","Raccord de réduction diam. ext. 35.28",10.43,10]
[null,"RR - 42.15","Raccord de réduction diam. ext. 42.15",26.51,4]
[null,"RR - 42.18","Raccord de réduction diam. ext. 42.18",26.82,4]
[null,"RR - 42.22","Raccord de réduction diam. ext. 42.22",18.48,4]
[null,"RR - 42.28","Raccord de réduction diam. ext. 42.28",18.950000000000003,4]
[null,"RR - 42.35","Raccord de réduction diam. ext. 42.35",11,4]
[null,"RR - 54.15","Raccord de réduction diam. ext. 54.15",29.37,4]
[null,"RR - 54.18","Raccord de réduction diam. ext. 54.18",29.610000000000003,4]
[null,"RR - 54.22","Raccord de réduction diam. ext. 54.22",29.830000000000002,4]
[null,"RR - 54.28","Raccord de réduction diam. ext. 54.28",31.14,4]
[null,"RR - 54.35","Raccord de réduction diam. ext. 54.35",21.970000000000002,4]
[null,"RR - 54.42","Raccord de réduction diam. ext. 54.42",12.61,4]
[null,"RR - 76.42","Raccord de réduction diam. ext. 76.42",56.309999999999995,2]
[null,"RR - 76.54","Raccord de réduction diam. ext. 76.54",58.28,2]
[null,"RR - 89.54","Raccord de réduction diam. ext. 89.54",62.879999999999995,2]
[null,"RR - 89.76","Raccord de réduction diam. ext. 89.76",85.76,2]
[null,"RR - 108.54","Raccord de réduction diam. ext. 108.54",66.100000000000009,2]
[null,"RR - 108.76","Raccord de réduction diam. ext. 108.76",89.03,2]
[null,"RR - 108.89","Raccord de réduction diam. ext. 108.89",98.690000000000012,2]
[null,"C180  -15","Courbe à 180° diam. ext. 15",9.9499999999999993,1]
[null,"C180 - 18","Courbe à 180° diam. ext. 18",10.629999999999999,1]
[null,"C180 - 22","Courbe à 180° diam. ext. 22",13.76,1]
[null,"C180 - 28","Courbe à 180° diam. ext. 28",15.379999999999999,1]
[null,"CD - 15","Crosse d'évêque diam. ext. 15",17.59,1]
[null,"CD - 18","Crosse d'évêque diam. ext. 18",18.990000000000002,1]
[null,"CD - 22","Crosse d'évêque diam. ext. 22",20.540000000000003,1]
[null,"CD - 28","Crosse d'évêque diam. ext. 28",22.680000000000003,1]
[null,"TU - 15","Tube \"sanitaire\" diam. ext. 15",8.1,120]
[null,"TU - 18","Tube \"sanitaire\" diam. ext. 18",8.58,90]
[null,"TU - 22","Tube \"sanitaire\" diam. ext. 22",12.879999999999999,60]
[null,"TU - 28","Tube \"sanitaire\" diam. ext. 28",15.73,60]
[null,"TU - 35","Tube \"sanitaire\" diam. ext. 35",24.21,60]
[null,"TU - 42","Tube \"sanitaire\" diam. ext. 42",29.01,30]
[null,"TU - 54","Tube \"sanitaire\" diam. ext. 54",35.9,30]
[null,"TU - 76","Tube \"sanitaire\" diam. ext. 76",62.98,30]
[null,"TU - 89","Tube \"sanitaire\" diam. ext. 89",73.88000000000001,30]
[null,"TU - 108","Tube \"sanitaire\" diam. ext. 108",91.72,30]
[null,"TU - 15A","Tube \"air comprimé\" diam. ext. 15",6.5299999999999994,120]
[null,"TU - 18A","Tube \"air comprimé\" diam. ext. 18",6.6499999999999995,90]
[null,"TU - 22A","Tube \"air comprimé\" diam. ext. 22",8.2799999999999994,60]
[null,"TU - 28A","Tube \"air comprimé\" diam. ext. 28",10.31,60]
[null,"TU - 35A","Tube \"air comprimé\" diam. ext. 35",15.65,60]
[null,"TU - 42A","Tube \"air comprimé\" diam. ext. 42",18.66,30]
[null,"TU - 54A","Tube \"air comprimé\" diam. ext. 54",23.98,30]
[null,"TU - 76A","Tube \"air comprimé\" diam. ext. 76",34.199999999999996,30]
[null,"TU - 89A","Tube \"air comprimé\" diam. ext. 89",40.11,30]
[null,"TU - 108A","Tube \"air comprimé\" diam. ext. 108",50.4,30]
[null,"JT - 76","Joint EPDM pour raccords diam. 76",0.71020000000000005,3]
[null,"JT - 89","Joint EPDM pour raccords diam. 89",1.4900799999999998,3]
[null,"JT - 108","Joint EPDM pour raccords diam. 108",1.9939200000000004,3]
[null,"JS - 15","Joint à sécurité EPDM pour raccords diam. 15",0.22780000000000003,20]
[null,"JS - 18","Joint à sécurité EPDM pour raccords diam. 18",0.2412,20]
[null,"JS - 22","Joint à sécurité EPDM pour raccords diam. 22",0.30820000000000003,20]
[null,"JS - 28","Joint à sécurité EPDM pour raccords diam. 28",0.34840000000000004,10]
[null,"JS - 35","Joint à sécurité EPDM pour raccords diam. 35",0.37520000000000003,10]
[null,"JS - 42","Joint à sécurité EPDM pour raccords diam. 42",0.40200000000000002,5]
[null,"JS - 54","Joint à sécurité EPDM pour raccords diam. 54",0.61640000000000006,5]
[null,"JV - 15","Joint FKM pour raccords diam. 15",0.72360000000000013,20]
[null,"JV - 18","Joint FKM pour raccords diam. 18",0.75040000000000007,20]
[null,"JV - 22","Joint FKM pour raccords diam. 22",0.87100000000000011,20]
[null,"JV - 28","Joint FKM pour raccords diam. 28",0.95140000000000002,10]
[null,"JV - 35","Joint FKM pour raccords diam. 35",1.1658000000000002,10]
[null,"JV - 42","Joint FKM pour raccords diam. 42",1.6080000000000001,5]
[null,"JV - 54","Joint FKM pour raccords diam. 54",2.5996000000000001,5]
[null,"JV - 76","Joint FKM pour raccords diam. 76",2.8140000000000005,3]
[null,"JV - 89","Joint FKM pour raccords diam. 89",3.9932000000000003,3]
[null,"JV - 108","Joint FKM pour raccords diam. 108",5.9763999999999999,3]
[null,"JP - 15","Joint plat EPDM pour raccords diam. 15",1.25,20]
[null,"JP - 18","Joint plat EPDM pour raccords diam. 18",1.25,20]
[null,"JP - 22","Joint plat EPDM pour raccords diam. 22",1.68,20]
[null,"JP - 28","Joint plat EPDM pour raccords diam. 28",1.98,10]
[null,"JP - 35","Joint plat EPDM pour raccords diam. 35",2.2200000000000002,10]
[null,"JP - 42","Joint plat EPDM pour raccords diam. 42",2.56,5]
[null,"JP - 54","Joint plat EPDM pour raccords diam. 54",4.17,5]
[null,"JPV - 15","Joint plat FKM pour raccords diam. 15",1.25,20]
[null,"JPV - 18","Joint plat FKM pour raccords diam. 18",1.25,20]
[null,"JPV - 22","Joint plat FKM pour raccords diam. 22",1.68,20]
[null,"JPV - 28","Joint plat FKM pour raccords diam. 28",1.98,10]
[null,"JPV - 35","Joint plat FKM pour raccords diam. 35",2.2200000000000002,10]
[null,"JPV - 42","Joint plat FKM pour raccords diam. 42",2.56,5]
[null,"JPV - 54","Joint plat FKM pour raccords diam. 54",4.17,5]
[null,"CL - 15","Collier protégé pour tube diam. 15 - M8",1.6428571428571428,100]
[null,"CL - 18","Collier protégé pour tube diam. 18 - M8",1.6785714285714284,100]
[null,"CL - 22","Collier protégé pour tube diam. 22 - M8",1.857142857142857,100]
[null,"CL - 28","Collier protégé pour tube diam. 28 - M8",1.8928571428571428,100]
[null,"CL - 35","Collier protégé pour tube diam. 35 - M8",2,100]
[null,"CL - 42","Collier protégé pour tube diam. 42 - M8",2.214285714285714,100]
[null,"CL - 54","Collier protégé pour tube diam. 54 - M8",2.464285714285714,100]
[null,"CL - 76","Collier protégé pour tube diam. 76 - M8",3.5714285714285712,50]
[null,"CL - 89","Collier protégé pour tube diam. 89 - M8",3.8571428571428572,50]
[null,"CL - 108","Collier protégé pour tube diam. 108 - M8",4.4285714285714279,50]
[null,"CLI - 15","Collier inox pour tube diam. 15 - M8",12.16,20]
[null,"CLI - 18","Collier inox pour tube diam. 18 - M8",12.16,20]
[null,"CLI - 22","Collier inox pour tube diam. 22 - M8",12.24,20]
[null,"CLI - 28","Collier inox pour tube diam. 28 - M8",12.45,10]
[null,"CLI - 35","Collier inox pour tube diam. 35 - M8",12.54,10]
[null,"CLI - 42","Collier inox pour tube diam. 42 - M8",12.74,10]
[null,"CLI - 54","Collier inox pour tube diam. 54 - M8",13.1,10]
[null,"CLI - 76","Collier inox pour tube diam. 76 - M8",17.010000000000002,5]
[null,"CLI - 89","Collier inox pour tube diam. 89 - M8",20.170000000000002,5]
[null,"CLI - 108","Collier inox pour tube diam. 108 - M8",30.19,5]
[null,"PV - M8","Patte à vis M 8 X 80",0.4,100]
[null,"TF - M8","Tige filetée M8 d'une longueur de 2 mètres",2.964285714285714,50]
[null,"CSJ - M8","Crampon serre joint de fixation M8",3.64,50]
[null,"SHE2","Sertisseuse electrique - 230V - 15-54mm",994,"Coffret"]
[null,"SHB3L","Sertisseuse electrique - batterie Li-On 18V - 15-54mm",1513,"Coffret"]
[null,"SHB4L","Sertisseuse electrique - batterie Li-On 18V - 15-108mm",2078,"Coffret"]
[null,"MDN 15","Mors DN 15 pour SHE2/SHB3L/SHB4L",102,"unitaire"]
[null,"MDN 18","Mors DN 18 pour SHE2/SHB3L/SHB4L",102,"unitaire"]
[null,"MDN 22","Mors DN 22 pour SHE2/SHB3L/SHB4L",102,"unitaire"]
[null,"MDN 28","Mors DN 28 pour SHE2/SHB3L/SHB4L",109,"unitaire"]
[null,"MDN 35","Mors DN 35 pour SHE2/SHB3L/SHB4L",130,"unitaire"]
[null,"CM5","Coffret metallique pour mors 15 à 35",110,"Coffret"]
[null,"CM5C","Coffret CM5 complet",655,"Coffret"]
[null,"CSK","Coffret Chaînes 42&54mm + adaptateur pour SHE/SHB",1280,"Coffret"]
[null,"CSB76","Chaînes DN76 pour SHB4L",1117,"Coffret"]
[null,"CSB89","Chaînes DN89 pour SHB4L",1150,"Coffret"]
[null,"CSB108","Chaînes DN108 pour SHB4L",1317,"Coffret"]
[null,"MICS4","Mors adaptateur  pour SHB4L",484,"Coffret"]
[null,"BS3L","Batterie supplémentaire Li-On 18V 3A",194,"unitaire"]
[null,"CRBL18V","Chargeur rapide 18V",137,"unitaire"]
[null,"AS18/230","Adaptateur secteur pour SHB3L/SHB4L",237,"unitaire"]
[null,"ETALONNEUR","Etalonneur",1.1100000000000001,"unitaire"]
[null,"SDP 1","Kit coupe tube 15-54 + ebavureur +  3 molettes",200,"Pack"]
[null,"MCI","Molette pour coupe tube serie CT",6.1,"unitaire"]
[null,"CT 76-108","Coupe tube manuelle pour diamètre 76mm à 108mm",155,"unitaire"]
[null,"CENTO","Coupe  tube éléctrique 22-108mm",876,"unitaire"]
[null,"MCC","Molette pour CENTO",56.7,"unitaire"]
[null,"SUPPCC","Support pour cento ",133,"unitaire"]
[null,"CHANDELLE CENTO","Chandelle pour CENTO",239.2,"unitaire"]